|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1. **Incident Name:**   **ATA North Rim Ramble** | | | | | **2. Date/Time Prepared:** Date: July 31, 2019 Time: 1830 MDT | | | | | | | **3. Operational Period:**  Date From: Aug. 25, 2019 Date To: Aug. 25, 2019 Time From: 0700 Time To: | | | |
| **4. Basic Radio Channel Use:** | | | | | | | | | | | | | | | |
| Zone Grp. | Ch # | Function | Channel Name/Trunked Radio System Talkgroup | | | Assignment | | RX Freq N or W | RX Tone/NAC | TX Freq N or W | TX Tone/NAC | | Mode (A, D, or M) | Remarks | |
|  | 1 | Operations | CARC | | | CARC Hams | | 146.4800 W | None | 146.4800 W | None | | A | Controlled Net | |
|  | 2 | Priority and Emergency Requests | Emergency 1 | | | Net Control | | 5.4035 USB | None | 5.4035 USB | None | | A | Comms with Flagstaff | |
|  | 3 | Priority and Emergency Requests | Emergency 2 | | | Net Control | | 5.3715 USB | None | 5.3715 USB | None | | A | Comms with Flagstaff | |
|  | 4 | Priority and Emergency Requests | Emergency 3 | | | Net Control | | 3.9900 LSB | None | 3.9900 LSB | None | | A | 75 meter backup for comms with Flagstaff | |
|  |  |  |  | | |  | |  |  |  |  | |  |  | |
|  |  |  |  | | |  | |  |  |  |  | |  |  | |
|  |  |  |  | | |  | |  |  |  |  | |  |  | |
|  |  |  | ­­­­ | | |  | |  |  |  |  | |  |  | |
| **5. Special Instructions:**  **Channel 1 stations require minimum 25 watt output and quality antennas. Handheld radios and “rubber duck” antennas are insufficient.**  **Channel 4 is approximate frequency. QRM may require actual frequency to be + or - 3.9900.**  **W7LUX, Joe Hobart is the primary contact for the emergency channels 2-4. Joe will be in Flagstaff, AZ.** | | | | | | | | | | | | | | | |
| **6. Prepared by** (Communications Unit Leader)**:** Name: Tom Shehan, KY7WV Signature: | | | | | | | | | | | | | | | |
| **ICS 205** | | | | | **IAP Page \_\_\_\_\_** | | | Date/Time: | | | | | | | |